|  |  |
| --- | --- |
| **In FVCOM43\_source:** | |
|  | |
| **Modified (7):** | |
| cntrl\_prmtrs.F | Added register function calling for surface output NetCDF file |
| mod\_input.F | a) Set the default values for the namelist NML\_NETCDF\_SURFACE  b) Added the code to check the direction of variable NV |
| mod\_main.F | Added definition and allocation of the surface variables for NetCDF output  Added the namelist NML\_NETCDF\_SURFACE for surface variable output |
| mod\_ncdio.F | Added new code for surface output NetCDF file |
| mod\_nesting.F | Modified the nesting input for hydrostatic mode |
| mod\_set\_time.F | Set the output time for the surface output file |
| mod\_utils.F | Added parameter NCSF\_CODE for surface variable output in MPI IO mode |